|  |  |
| --- | --- |
| N | **Requirements** |
| 1 | Compact( no need for PC) and portable digital flow meter) |
| 2 | Accuracy+\-3% of the actual value |
| 3 | Calibration and equilibration software, automatic equilibration |
| 4 | Maximum load capacity of the sensor unit 1000g |
| 5 | Measurement start, measurement end choice of automatic or manual |
| 6 | Built in the thermal printer |
|  | High precision weighing unite with stand |