Requested Quantity : 3 Central RO Unit includes :

1. Pre filter to remove particulates greater than 5 microns.
2. Stainless steel Pump and Automatic Flushing.
3. Pressure Adjust regulator and gauges.
4. inlet water sensor to monitors the quality of the inlet water.
5. Automatic softener and carbon filter compatible with RO System.
6. Disinfectant port.
7. TDS display monitor and Pressure Gauges.
8. RO Pump Power Switch is mounted on the front panel.
9. FDA registered manufacturer meets stringent medical devices requirements.

\*\* Water Specification Required :

|  |  |
| --- | --- |
| TDS | : not more than 10 ppm |
| TH | : Zero |
| Production Rate : > 350 L/hr | |
| 'h k | Hospital Water : |
| TDS | : 400 ppm |
| TH | : 100 ppm |
| Cl | : 0.4 ppm |
|  |  |