|  |  |  |
| --- | --- | --- |
| **No.** | **Technical Specifications** | **Min KAUH Requirement** |
| 1 | Manufacturer | Please specify manufacturer and country of origin |
| 2 | Model Number | Please specify model number of the offered equipment |
| 3 | Safety Standard | FDA approval or CE marking |
| 4 | Main features | * **One-demand Cassettes printing** * Precise,clean and High resolution print out * Permanent (Resistance to histological chemicals) * Enables patch mode printing * Low noise printer * Compatible with regular cassettes in the market * Accepts scanner for instant cassette scanning * Enables black printing |
| 5 | Character type | * Numeric graphic and logo printing and barcode |
| 6 | Printing technology | Laser or thermal |
| 7 | Through put | To be mentioned |
| 8 | Number of hopper | Not less than two |
| 9 | Printing speed | < 10 seconds/ cassette |
| 10 | capacity | >150 cassettes |
| 11 | software | Permanent license |
| 12 | Main Power | 220-240Vac 50 Hz |