**Technical Specifications for - Washer Machine Qty (1)**

|  |  |  |
| --- | --- | --- |
| **No.** | **Technical Specifications** | **Min KAUH Requirement** |
| 1 | Manufacturer | Please specify manufacturer and country of origin |
| 2 | Model Number | Please specify model number of the offered equipment |
| 3 | Main Specifications | * 3- Phase, 380 V, 50 Hz
* Automatic Washer Extractor
* ( Double Door Front & Back Side )
* Microprocessor Controller
* Multi Functions
* Material : Stainless Steel 304 ( Drum, Tube & Cabinet )
* Standard Liquid Soap Connection
* Cold & Hot Water Connections
* Direct Steam Heated
* Safety Door Locking System
* Emergency Stop
 |
| 4 | Capacity | * 40 – 60 Kgs.
 |
| 5 | Washing Speed  | > 30 rpm |
| 6 | Spin Speed  | 350 - 700 rpm. |
| 7 | Steam Pressure  | 4 – 6 bar |
| 8 | Comp. Air  | 4 – 6 bar |

|  |
| --- |
|  |

**الموضوع: المواصفات الفنية لأجهزة المصبغه**

**Technical Specifications for - Washer Machine Qty (4)**

|  |  |  |
| --- | --- | --- |
| **No.** | **Technical Specifications** | **Min KAUH Requirement** |
| 1 | Manufacturer | Please specify manufacturer and country of origin |
| 2 | Model Number | Please specify model number of the offered equipment |
| 3 | Main Specifications | * 3- Phase, 380 V, 50 Hz
* Automatic Single Door Front Side Washing Machine
* Microprocessor Controller
* Multi Functions
* Material : Stainless Steel 304 ( Drum, Tube & Cabinet )
* Standard Liquid Soap Connection
* Cold & Hot Water Connections
* Direct Steam Heated
* Safety Door Locking System
* Emergency Stop
 |
| 4 | Capacity | 100 – 120 Kgs. |
| 5 | Washing Speed  | > 30 rpm |
| 6 | Spin Speed  | 350 - 700 rpm. |
| 7 | Steam Pressure  | 4 – 6 bar |
| 8 | Comp. Air  | 4 – 6 bar |

|  |
| --- |
|  |
|  |

**الموضوع: المواصفات الفنية لأجهزة المصبغه**

**Technical Specifications for - Dryer Machine Qty (2)**

|  |  |  |
| --- | --- | --- |
| **No.** | **Technical Specifications** | **Min KAUH Requirement** |
| 1 | Manufacturer | Please specify manufacturer and country of origin |
| 2 | Model Number | Please specify model number of the offered equipment |
| 3 | Main Specifications | * 3- Phase , 380 V, 50 Hz
* Steam Heated
* Stainless Steel Drum
* Front Door Loading
* Reverse System
 |
| 4 | Capacity | > 70 kgs. |
| 7 | Steam Pressure  | 4 – 6 bar |
| 8 | Air Pressure  | 4 – 6 bar |

**الموضوع: المواصفات الفنية لأجهزة المصبغه**

**Technical Specifications for - Stainless Steel Lint Collector Qty (1)**

|  |  |  |
| --- | --- | --- |
| **No.** | **Technical Specifications** | **Min KAUH Requirement** |
| 1 | Manufacturer | Please specify manufacturer and country of origin |
| 2 | Model Number | Please specify model number of the offered equipment |
| 3 | Main Specifications |  Compatible with capacity 6 Drayers Machine Total Capacity for All Drayers 360 - 400 Kgs / Hour |

**الموضوع: المواصفات الفنية لأجهزة المصبغه**

**Technical Specifications for - Press Machine Qty (1)**

|  |  |  |
| --- | --- | --- |
| **No.** | **Technical Specifications** | **Min KAUH Requirement** |
| 1 | Manufacturer | Please specify manufacturer and country of origin |
| 2 | Model Number | Please specify model number of the offered equipment |
| 3 | Main Specifications | * 3- Phase ,380 V, 50 Hz
* Air operated press utility shape
* Over All Dimension 1400 X 1150 X 1400 mm

  |
| 4 | Steam inlet & Return outlet | ½ inch |
| 5 | Air inlet  | 3/8 inch |
| 6 | Steam working Pressure | 5 Bar |
| 7 | Air Working Pressure  | 7 Bar |

**الموضوع: المواصفات الفنية لأجهزة المصبغه**

**Technical Specifications for - Ironing & Folder Machine Qty (1)**

|  |  |  |
| --- | --- | --- |
| **No.** | **Technical Specifications** | **Min KAUH Requirement** |
| 1 | Manufacturer | Please specify manufacturer and country of origin |
| 2 | Model Number | Please specify model number of the offered equipment |
| 3 | Main Specifications | * 3- Phase ,380 V, 50 Hz
* Pulse folding with up to two primary folds and three cross folds
* Digital Temp. display and steam pressure gauge monitor heating system
* Dependable Rotary steam union
* Admits steam and discharges condensate
* Fully automatic
* Multi Function
* LCD Screen Display
* Emergency Stop
* Infrared Ray to detected and count
* Anti static device
 |
| 4 | Steam working Pressure | 6-10 Bar |
| 5 | Ironing Width not less than  | 3000 mm |
| 6 | Ironing Speed  | 4 – 36 m/min |
| 7 | Heating Type | Steam |
| 8 | No. of Rolls  | 1 |
| 9 | Folding Width  |  |