**Technical Specifications for - Washer Machine Qty (1)**

|  |  |  |
| --- | --- | --- |
| **No.** | **Technical Specifications** | **Min KAUH Requirement** |
| 1 | Manufacturer | Please specify manufacturer and country of origin |
| 2 | Model Number | Please specify model number of the offered equipment |
| 3 | Main Specifications | * 3- Phase, 380 V, 50 Hz * Automatic Washer Extractor * ( Double Door Front & Back Side ) * Microprocessor Controller * Multi Functions * Material : Stainless Steel 304 ( Drum, Tube & Cabinet ) * Standard Liquid Soap Connection * Cold & Hot Water Connections * Direct Steam Heated * Safety Door Locking System * Emergency Stop |
| 4 | Capacity | * 40 – 60 Kgs. |
| 5 | Washing Speed | > 30 rpm |
| 6 | Spin Speed | 350 - 700 rpm. |
| 7 | Steam Pressure | 4 – 6 bar |
| 8 | Comp. Air | 4 – 6 bar |

|  |
| --- |
|  |

**الموضوع: المواصفات الفنية لأجهزة المصبغه**

**Technical Specifications for - Washer Machine Qty (4)**

|  |  |  |
| --- | --- | --- |
| **No.** | **Technical Specifications** | **Min KAUH Requirement** |
| 1 | Manufacturer | Please specify manufacturer and country of origin |
| 2 | Model Number | Please specify model number of the offered equipment |
| 3 | Main Specifications | * 3- Phase, 380 V, 50 Hz * Automatic Single Door Front Side Washing Machine * Microprocessor Controller * Multi Functions * Material : Stainless Steel 304 ( Drum, Tube & Cabinet ) * Standard Liquid Soap Connection * Cold & Hot Water Connections * Direct Steam Heated * Safety Door Locking System * Emergency Stop |
| 4 | Capacity | 100 – 120 Kgs. |
| 5 | Washing Speed | > 30 rpm |
| 6 | Spin Speed | 350 - 700 rpm. |
| 7 | Steam Pressure | 4 – 6 bar |
| 8 | Comp. Air | 4 – 6 bar |

|  |
| --- |
|  |
|  |

**الموضوع: المواصفات الفنية لأجهزة المصبغه**

**Technical Specifications for - Dryer Machine Qty (2)**

|  |  |  |
| --- | --- | --- |
| **No.** | **Technical Specifications** | **Min KAUH Requirement** |
| 1 | Manufacturer | Please specify manufacturer and country of origin |
| 2 | Model Number | Please specify model number of the offered equipment |
| 3 | Main Specifications | * 3- Phase , 380 V, 50 Hz * Steam Heated * Stainless Steel Drum * Front Door Loading * Reverse System |
| 4 | Capacity | > 70 kgs. |
| 7 | Steam Pressure | 4 – 6 bar |
| 8 | Air Pressure | 4 – 6 bar |

**الموضوع: المواصفات الفنية لأجهزة المصبغه**

**Technical Specifications for - Stainless Steel Lint Collector Qty (1)**

|  |  |  |
| --- | --- | --- |
| **No.** | **Technical Specifications** | **Min KAUH Requirement** |
| 1 | Manufacturer | Please specify manufacturer and country of origin |
| 2 | Model Number | Please specify model number of the offered equipment |
| 3 | Main Specifications | Compatible with capacity 6 Drayers Machine  Total Capacity for All Drayers 360 - 400 Kgs / Hour |

**الموضوع: المواصفات الفنية لأجهزة المصبغه**

**Technical Specifications for - Press Machine Qty (1)**

|  |  |  |
| --- | --- | --- |
| **No.** | **Technical Specifications** | **Min KAUH Requirement** |
| 1 | Manufacturer | Please specify manufacturer and country of origin |
| 2 | Model Number | Please specify model number of the offered equipment |
| 3 | Main Specifications | * 3- Phase ,380 V, 50 Hz * Air operated press utility shape * Over All Dimension 1400 X 1150 X 1400 mm |
| 4 | Steam inlet & Return outlet | ½ inch |
| 5 | Air inlet | 3/8 inch |
| 6 | Steam working Pressure | 5 Bar |
| 7 | Air Working Pressure | 7 Bar |

**الموضوع: المواصفات الفنية لأجهزة المصبغه**

**Technical Specifications for - Ironing & Folder Machine Qty (1)**

|  |  |  |
| --- | --- | --- |
| **No.** | **Technical Specifications** | **Min KAUH Requirement** |
| 1 | Manufacturer | Please specify manufacturer and country of origin |
| 2 | Model Number | Please specify model number of the offered equipment |
| 3 | Main Specifications | * 3- Phase ,380 V, 50 Hz * Pulse folding with up to two primary folds and three cross folds * Digital Temp. display and steam pressure gauge monitor heating system * Dependable Rotary steam union * Admits steam and discharges condensate * Fully automatic * Multi Function * LCD Screen Display * Emergency Stop * Infrared Ray to detected and count * Anti static device |
| 4 | Steam working Pressure | 6-10 Bar |
| 5 | Ironing Width not less than | 3000 mm |
| 6 | Ironing Speed | 4 – 36 m/min |
| 7 | Heating Type | Steam |
| 8 | No. of Rolls | 1 |
| 9 | Folding Width |  |